[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring SRC ACP (C-Web Interface)

To use SRC Admission Control Plug-In (ACP) in the SRC network, you must perform some configuration. For information about these configuration procedures, see:

1. (Optional) Configure a grouped configuration for SRC ACP.
2. Configuring Local Properties for SRC ACP (C-Web Interface)
3. Configuring the SAE for SRC ACP (C-Web Interface)
4. Configuring SRC ACP Properties (C-Web Interface)
5. (Edge and dual mode only) Configuring SRC ACP to Manage the Edge Network (C-Web Interface)
6. (Backbone and dual mode only) Configuring SRC-ACP to Manage the Backbone Network (C-Web Interface)

You can automate and scale the configuration of congestion points using congestion point classification. For more information, see Configuring NIC Test Data (SRC CLI) and Configuring Congestion Point Classification (C-Web Interface).

#### Related Topics

- Configuring ACP to Store Log Messages in a File (C-Web Interface)
- Overview of SRC ACP

[Contents] [Prev] [Next] [Index] [Report an Error]