> - Downloads
> - Specifying the PCMM Classifier Type (C-Web Interface)
> - Related Topics
> - Before You Configure Classify-Traffic Conditions
> - Delivering QoS Services in a Cable Environment
> - Configuring Classify-Traffic Conditions (C-Web Interface)
> - Specifying the PCMM Classifier Type (SRC CLI)

> # Specifying the PCMM Classifier Type (C-Web Interface)

> To specify whether or not the SAE sends to the router classifiers that comply with PCMM I03:

> 1. Select Configure, expand Shared>SAE>Configuration>Driver, and select pcmm.
> 2. Check or clear the Disable PCMM I03 Policy box, and click Apply.

> #### Published: 2009-09-18

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.