[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring the SAE to Manage AAA Devices

Use the following configuration statements to configure the AAA device driver:

`

shared sae configuration driver aaa {
  sae-community-manager sae-community-manager;
  origin-host origin-host;
  origin-realm origin-realm;
  keep-alive-timeout keep-alive-timeout;
  registry-retry-interval registry-retry-interval;
  reply-timeout reply-timeout;
  sequential-message-timeout sequential-message-timeout;
  transient-session-timeout transient-session-timeout;
  max-update-interval max-update-interval;
  update-grace-period update-grace-period;
  resume-unrecovered;
  thread-pool-size thread-pool-size;
  thread-idle-timeout thread-idle-timeout;
}

`

To configure the AAA device driver:

1. From configuration mode, access the configuration statements for the AAA device driver.
   `
   user@host# edit shared sae configuration driver aaa
   `
2. Specify the name of the community manager.
   `
   [edit shared sae configuration driver aaa]
   user@host# set sae-community-manager sae-community-manager
   `
3. (Optional) Specify the fully qualified domain name used to identify this host.
   `
   [edit shared sae configuration driver aaa]
   user@host# set origin-host origin-host
   `
4. (Optional) Specify the DNS name of the machine used to identify this host.
   `
   [edit shared sae configuration driver aaa]
   user@host# set origin-realm origin-realm
   `
5. (Optional) Specify the keepalive timeout before the registry to a Diameter server expires.
   `
   [edit shared sae configuration driver aaa]
   user@host# set keep-alive-timeout keep-alive-timeout
   `
6. (Optional) Specify the interval between retrying a failed registry to a Diameter server.
   `
   [edit shared sae configuration driver aaa]
   user@host# set registry-retry-interval registry-retry-interval
   `
7. (Optional) Specify the timeout before a request sent to a Diameter server expires.
   `
   [edit shared sae configuration driver aaa]
   user@host# set reply-timeout reply-timeout
   `
8. (Optional) Specify the timeout before an expected message expires.
   `
   [edit shared sae configuration driver aaa]
   user@host# set sequential-message-timeout sequential-message-timeout
   `
9. (Optional) Specify the timeout before a temporary session expires.
   `
   [edit shared sae configuration driver aaa]
   user@host# set transient-session-timeout transient-session-timeout
   `
10. (Optional) Specify the maximum interval between interim updates for a subscriber session.
    `
    [edit shared sae configuration driver aaa]
    user@host# set max-update-interval max-update-interval
    `
11. (Optional) Specify the grace period in which to expect an interim update for a subscriber session.
    `
    [edit shared sae configuration driver aaa]
    user@host# set update-grace-period update-grace-period
    `
12. (Optional) Specify whether to resume a subscriber session that has failed to recover from a failover.
    `
    [edit shared sae configuration driver aaa]
    user@host# set resume-unrecovered
    `
13. (Optional) Specify the number of working threads that process requests.
    `
    [edit shared sae configuration driver aaa]
    user@host# set thread-pool-size thread-pool-size
    `
14. (Optional) Specify the timeout for stopping working threads after they become idle.
    `
    [edit shared sae configuration driver aaa]
    user@host# set thread-idle-timeout thread-idle-timeout
    `
15. (Optional) Configure the session store parameters for the AAA device driver.

    From configuration mode, access the configuration statement that configures the session store for the AAA device driver.

    `
    user@host# edit shared sae configuration driver aaa session-store
    `

    For more information about configuring session store parameters, see Configuring the Session Store Feature.

[Contents] [Prev] [Next] [Index] [Report an Error]