[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring the SAE to Manage PCMM Devices (C-Web Interface)

The SAE connects to the PCMM device by using a COPS over TCP connection. The PCMM device driver controls this connection.

To configure the SAE to manage PCMM devices:

1. Click Configure, expand Shared>SAE>Configuration>Driver, and then click PCCM.

   The PCCM pane appears.

2. Click Create, enter information as described in the Help text in the main pane, and then click Apply.

#### Related Topics

- For information about setting up SAE groups, see Setting Up an SAE with the C-Web Interface
- Configuring the SAE to Manage PCMM Devices (SRC CLI)
- Configuring PCMM Record-Keeping Server Plug-Ins (SRC CLI)
- Using the SAE in a PCMM Environment

[Contents] [Prev] [Next] [Index] [Report an Error]