[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring RADIUS Authentication (C-Web Interface)

To configure information about RADIUS servers for authentication:

1. Click Configure>System.

   The System pane appears.

2. From the Create new list, select RADIUS Server.
3. Type an IPv4 address or IPv6 address in the dialog box, and click OK.

   The RADIUS Server pane appears.

4. Enter information as described in the Help text in the main pane, and click Apply.

To configure a set of users that share a single account for authorization purposes, you create a template user.

#### Related Topics

- Configuring RADIUS Authentication (SRC CLI)
- Configuring RADIUS and TACACS+ Authentication on a C Series Controller (C-Web Interface)
- Configuring Authentication Order
- Removing an Authentication Method from the Authentication Order

[Contents] [Prev] [Next] [Index] [Report an Error]