> - Downloads
> - Configuring Subscriber IP Pools as IP Subnets (C-Web Interface)
> - Related Topics
> - Configuring Subscriber IP Pools as IP Subnets
> - Configuring Subscriber IP Pools as IP Address Ranges (C-Web Interface)
> - Modifying the Subscriber Configuration (C-Web Interface)

> # Configuring Subscriber IP Pools as IP Subnets (C-Web Interface)

> To configure subscriber IP pools that are managed by the CMTS device as IP subnets:

> 1. Click Configure, expand Slot>Slot: 0>JPS, and then click CMTS Registry.

>    The CMTS Registry pane appears.

> 2. From the Create new list, select CMTS.
> 3. In the dialog box, type an IPv4 or IPv6 address for the new CMTS, and click OK.

>    The CMTS:<ip address> pane appears.

> 4. From the Create new list, select Subnet Pool.
> 5. In the dialog box, enter a network IP address/mask for the new Subnet Pool, and click OK.

>    The Subnet Pool: <ip address/mask> pane appears.

> 6. Enter the information in the main pane as described in the Help text, and click Apply.

> #### Published: 2009-09-18

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.