[Contents] [Prev] [Next] [Index] [Report an Error]

# Changing the Location of Data in the Directory

In most cases, you use the default configuration for the location of SRC data in the directory:

- Administrator-defined configuration data—ou=staticConfiguration,ou=Configuration,o=Management,o=umc
- Programmatically defined configuration data—ou=dynamicConfiguration,ou=Configuration,o=Management, o=umc

You can specify the full distinguished name (DN), or a DN relative to a base DN, identified as <base>.

You can change the location of data in the directory at the Expert CLI editing level.

Use the following configuration statements to change the location of data for a component in the directory:

`

slot number component-name initial {
  static-dn static-dn ;
  dynamic-dn dynamic-dn ;
}

`

To change the location of data in the directory:

1. From configuration mode, access the configuration statement that specifies the configuration for a component on a slot.
   `
   [edit]
   user@host# edit slot number nic initial
   `

   For example:

   `
   [edit]
   user@host# edit slot 0 nic initial
   `
2. (Optional) Change the location of administrator-defined configuration data in the directory
   `
   [edit slot 0 nic initial]
   user@host# set static-dn static-dn
   `
3. (Optional) Change the location of programmatically defined configuration data in the directory.
   `
   [edit slot 0 nic initial]
   user@host# set dynamic-dn dynamic-dn
   `

#### Related Topics

- Configuring Initial Directory Eventing Properties for SRC Components
- Configuring Basic Local Properties
- Configuration Statements for Local Configuration
- Managing Directory Communication

[Contents] [Prev] [Next] [Index] [Report an Error]