[Contents] [Prev] [Next] [Index] [Report an Error]

## Index

A B C D E F G H I J L M N O P R S T U V

A

> access DNs 1
> accounting
>   SAE, description 1
> ACP (Admission Control Plug-In)
>   redundancy
>     monitoring 1
> ACP. See SRC ACP
> action congestion points 1
>   configuring 1
>   monitoring
>     C-Web interface 1, 2
>     SRC CLI 1, 2
> address pools. See IP address pools
> Admission Control Plug-In. See SRC ACP
> agents See NIC agents
> allocating bandwidth to applications not controlled by SRC ACP 1
> APIs
>   SRC ACP 1
> APIs (application programming interfaces)
>   CORBA remote API 1
>   NIC 1
>   provided with SAE 1
>   SAE core API 1
> application programming interfaces. See APIs
> applications
>   executing with SRC ACP 1
>   external for use with SRC ACP 1, 2
> assigned IP subscribers
>   third-party devices 1
>     IP address pools 1
> assigning
>   edge congestion points to subscribers 1
>   interfaces to backbone congestion point profiles 1
>   interfaces to subscribers 1
> ATM access network, using with SRC ACP 1
> authorizing and tracking services 1

B

> backbone congestion point profiles
>   configuring 1
> backbone congestion points 1
>   configuring 1
>   configuring for services 1
>   defining applications in 1
>   deriving 1
>   DNs of 1
>   monitoring
>     SRC CLI 1, 2
>   running applications from 1
> backbone network 1
> backbone network management with SRC ACP
>   configuring 1
> background bandwidth 1
> bandwidth
>   allocating to applications not controlled by SRC ACP 1
>   background 1, 2
>   configuring
>     for services 1, 2
>     for subscribers 1
>   downstream 1
>   upstream 1
> bandwidths and congestion points for subscribers
>   configuring 1
> BEEP, JUNOS routing platforms 1
>   configuring port
>     SRC CLI 1
>   connection 1
> Blocks Extensible Exchange Protocol. See BEEP

C

> certificate authority (CA) 1
> classification scripts
>   congestion point classification
>     configuring 1
>     criteria 1, 2
>     description 1
>     how it works 1
>     targets 1, 2
> Common Object Request Broker Architecture. See CORBA
> community manager
>   configuring, third-party devices
>     SRC CLI 1
> component interactions
>   JUNOS routing platforms and SAE 1
> configuration group, JUNOS routing platforms 1, 2
> configuration manager, instantiating for NIC 1
> congestion point applications
>   SPI for ACP 1
> congestion point classification 1, 2
> congestion point classification scripts. See classification scripts
> congestion point expressions 1, 2
> congestion point profiles 1
>   congestion point expressions 1
>   defining 1
> congestion points 1, 2
>   configuring 1
>   defining applications in 1
>   deriving 1
>   deriving from congestion point expressions 1
>   deriving from profile 1
>   managing 1
>   modifying 1
>   monitoring 1, 2
>   retrieving information about 1
> conventions
>   notice icons 1
>   text 1
> COPS (Common Open Policy Service)
>   connection with JUNOSe routers 1
>     configuring SAE, SRC CLI 1
>     disabling on router 1
>     enabling on router 1
>   COPS-PR versus COPS XDR 1
>   JUNOSe router connection 1
> CORBA (Common Object Request Broker Architecture)
>   IOR location 1
>   remote API 1
> CORBA interfaces
>   SRC ACP 1
> CORBA-based plug-in SPI. See plug-ins, external
> customer support 1
>   contacting JTAC 1
> customized interface modules 1

D

> deriving congestion points 1
> device drivers
>   JUNOS
>     configuring, SRC CLI 1
>     viewing state, C-Web interface 1
>     viewing state, SRC CLI 1
>     viewing statistics, C-Web interface 1, 2
>     viewing statistics, SRC CLI 1, 2
>   JUNOSe
>     configuring, SRC CLI 1
>     viewing state, C-Web interface 1
>     viewing statistics, SRC CLI 1, 2
> directory
>   services for SRC ACP 1
>   subscribers for SRC ACP 1
> directory blacklist, deleting 1, 2
> distinguished name. See DN
> DN (distinguished name)
>   NIC resolution 1
> DNs
>   backbone congestion points 1
>   edge congestion points 1
> documentation
>   comments on 1
> domain maps
>   reloading on SAE 1
> downstream bandwidth 1

E

> edge congestion points
>   assigning to subscribers 1
>   deriving 1
>   DNs of 1
>   monitoring
>     SRC CLI 1, 2
> edge network 1, 2
> edge network management, configuring 1
> equipment registration
>   deleting 1, 2
> event notification, PCMM network
>   configuration statements 1
>   properties, configuring
>     SRC CLI 1
> event notification, third-party devices
>   description 1
> events, publishing 1
> external applications
>   displaying information from 1
>   interaction with NIC 1
>   monitoring
>     C-Web interface 1, 2
> external plug-ins
>   configuring SRC ACP as 1
> external plug-ins. See plug-ins
> External Subscriber Monitor
>   acting as pseudo RADIUS server, C-Web interface 1
>   agent process statistics, viewing
>     SRC CLI 1
>   configuring 1
>   configuring basic local properties 1
>   configuring client secret 1
>   configuring directory connection properties 1
>   configuring event notification 1
>   configuring eventing properties 1
>   configuring initial properties 1
>   configuring logging destinations 1
>   event notifications, monitoring
>     SRC CLI 1
>   event notifications, viewing
>     SRC CLI 1
>   IP address manager 1
>     C-Web Interface 1
>   overview, C-Web interface 1
>   starting 1
>   statistics, monitoring
>     SRC CLI 1
>   statistics, viewing
>     SRC CLI 1
>   stopping 1

F

> failover parameters, SAE 1, 2
> fault recovery, SRC ACP 1
> files
>   ACP data 1

G

> groups, NIC hosts 1

H

> hosted internal plug-in 1
> hosted plug-ins. See plug-ins

I

> interactions between SRC ACP and other components 1, 2
> interface classification scripts
>   reloading on SAE 1, 2
> interface modules, SAE 1
> interfaces, assigning to backbone congestion point profiles 1
> internal plug-ins. See plug-ins
> IOR
>   router initialization scripts 1, 2
> IP address pools
>   local address pools, configuring
>     SRC CLI 1, 2
>   static pools, configuring
>     SRC CLI 1, 2

J

> JUNOS routing platforms
>   BEEP connection 1
>     configuring port, SRC CLI 1
>   configuration groups 1, 2
>   configuring to interact with SAE 1
>   default virtual router 1
>   disabling interactions with SAE 1
>   enabling interactions with SAE 1
>   monitoring interactions with SAE 1
>   SAE interactions 1
>   SRC software process 1
>   troubleshooting 1
> JUNOSe routers
>   accessing router CLI 1
>   COPS connection 1
>     configuring, SRC CLI 1
>   integration overview 1
>   monitoring interactions with SAE 1
>   router objects, adding
>     SRC CLI 1
>   SRC client 1
>     starting 1
>     stopping 1
>   troubleshooting 1
>   VR objects
>     adding individually, SRC CLI 1, 2
>     discovering, SRC CLI 1

L

> LDAP access. See SAE (service activation engine), configuring
> logging properties
>   configuring for SRC ACP 1
> login names 1
> login process
>   assigned IP subscribers, third-party devices 1
>   event notification method, third-party devices 1
> login registration
>   deleting 1, 2

M

> managing
>   congestion points 1
>   edge network with SRC ACP 1
> manuals
>   comments on 1
> modifying congestion points 1
> monitoring
>   backbone congestion points 1
>   SRC ACP
>     C-Web interface 1
>     SRC CLI 1

N

> NAS port ID 1
> network information collector. See NIC
> network interfaces 1, 2
> network publisher See NIC
> NIC (network information collector) 1
>   API 1
>   configuration prerequisites
>     C Series Controllers 1
>   configuration statements 1
>   configuration, changing 1
>   configuration, verifying 1
>   data mapping 1
>   default operating properties, viewing 1
>   factory interface 1, 2
>   logging
>     changing configuration 1
>     default 1
>   monitors
>     example 1
>   network publisher
>     overview 1
>     prerequisites 1
>     running 1
>     troubleshooting 1
>   operating properties, changing 1
>   overview 1
>   planning implementation 1
>   realms
>     overview 1
>   replication
>     groups 1
>     overview 1
>     SAE plug-in agents 1
>   replication, configuring 1
>   resolution processes 1, 2
>   resolvers
>     constraints 1
>     overview 1
>   restarting 1
>   roles 1
>   starting 1
>   stopping 1
>   testing
>     any key 1
>     examples 1
>     resolution 1
>     test data 1
>   viewing
>     configuration 1
>   See also other NIC entries
> NIC agents
>   configuration overview 1
>   directory, configuring
>     SRC CLI 1
>   overview 1, 2
>   restarting 1
>   sae client agents, configuring 1
>   sae plug-in agents, configuring 1
> NIC configuration scenarios
>   changing 1
>     SRC CLI 1
>   Multipop 1
>   OnePop 1
>   OnePopAcctId 1
>   OnePopAllRealms 1
>   OnePopDnSharedIp 1
>   OnePopDynamicIp 1
>   OnePopLogin 1
>   OnePopLoginPull 1
>   OnePopPcmm 1
>   OnePopPrimaryUser 1
>   OnePopSharedIp 1
>   OnePopStaticRouteIp 1, 2
>   OnePopVrfIp 1, 2
>   overview 1, 2
>   scenario-name 1
> NIC hosts
>   configuration prerequisites 1
>   groups 1
>   overview 1
>   redundancy
>     example 1
>   starting 1
>   stopping 1, 2, 3, 4
> NIC locators
>   external applications 1, 2
>   overview 1, 2
> NIC proxies
>   cache, configuring
>     SRC CLI 1
>   configuration overview 1
>   configuration prerequisites 1
>   instantiating 1
>   logging 1
>   NIC replication, configuring
>     SRC CLI 1
>   overview 1
>   prerequisites 1
>   removing instances 1
>   requirements 1, 2
>   resolution information, configuring
>     SRC CLI 1
>   resolution requests 1
> NIC Proxy for Pseudo-RADIUS server
>   configuring 1
> NIC proxy for Pseudo-RADIUS server
>   changing configuration 1
>   configuring for NIC replication 1
>   configuring resolution 1
> NIC resolvers
>   restarting 1
> nic-network-publisher-configuration-statements 1
> notice icons 1

O

> operation
>   SRC ACP, configuring 1

P

> PacketCable Multimedia. See PCMM
> PCMM (PacketCable Multimedia)
>   SAE connection 1
> plug-ins
>   architecture 1
>   external 1
>   hosted 1
>   hosted internal plug-in 1
>   internal 1
>   SRC ACP 1
>   tracking
>     virtual routers, SRC CLI 1, 2
>   types 1
> preventing
>   service activation 1
> priorityList 1
> properties
>   SRC ACP 1
> pseudo-RADIUS server
>   configuring External Subscriber Monitor 1
> publishing events 1

R

> randomPick 1
> realm
>   See NIC realms
> redundancy, SRC ACP 1
> resolution processes
>   DN to SAE reference 1, 2, 3
>   IP address to login name 1
>   IP address to SAE reference 1, 2, 3, 4, 5, 6
>   login name to SAE reference 1
> roles, NIC 1
> roundRobin 1
> router initialization scripts
>   iorPublisher 1, 2
>   JUNOS
>     configuring location, SRC CLI 1
>   JUNOSe 1, 2
>     configuring location, SRC CLI 1
>     example 1, 2
>   poolPublisher 1, 2
>   specifying for NIC 1
> router object
>   adding for third-party devices
>     SRC CLI 1
> routers
>   accessing router CLI 1
>   adding JUNOS routing platforms
>     SRC CLI 1
>   adding JUNOSe
>     SRC CLI 1
>   integrating JUNOS routing platform 1
>   integrating JUNOSe 1

S

> SAE (service activation engine)
>   accounting 1
>   APIs. See APIs
>   BEEP connection, JUNOS routing platforms 1
>   COPS
>     JUNOSe router connection 1
>   deleting directory blacklist 1, 2
>   disabling interactions with JUNOS routing platform 1
>   enabling interactions with JUNOS routing platform 1
>   failover parameters 1, 2
>   JUNOS routing platform client 1
>   monitoring interactions
>     JUNOS routing platform 1
>     JUNOSe routers 1
>   NIC replication, configuring
>     SRC CLI 1
>   overview 1
>   PCMM environment 1
>   plug-ins See plug-ins
>   reloading configuration 1, 2, 3, 4
>   role 1
>   router initialization scripts. See router initialization scripts
>   session store
>     C Series Controllers 1
>   starting
>     SRC client on JUNOSe router 1
>   stopping
>     SRC client on JUNOSe router 1
> SAE (service activation engine), configuring
>   BEEP connection
>     SRC CLI 1
>   COPS connection
>     SRC CLI 1
>   directory eventing, SAE configuration data
>     SRC CLI 1
>   event notification API properties
>     SRC CLI 1
>   LDAP access, SRC CLI
>     device data 1
>     directory data 1
>     persistent login cache data 1
>     policy data 1
>     service data 1
>     subscriber data 1
>   router initialization script location
>     SRC CLI 1, 2
>   serialized data compression
>     SRC CLI 1
>   session job manager
>     SRC CLI 1
>   session store
>     SRC CLI 1
>   SRC ACP 1
> SAE (service activation engine),configuring
>   to monitor backbone congestion points 1
> SAE communities
>   configuring, third-party devices
>     SRC CLI 1
>   description, third-party devices 1
> SAE remote interface
>   customized interface modules 1
> script services
>   for third-party devices 1
> serialized data compression, configuring
>   SRC CLI 1
> service activation engine. See SAE
> services
>   configuring bandwidth for 1, 2
>   monitoring
>     C-Web interface 1
>     SRC CLI 1
>   preventing activation 1
>   reloading on SAE 1, 2
> session job manager, configuring
>   SRC CLI 1
> session store
>   C Series Controllers 1
>   configuring, SRC CLI
>     compressing session objects 1
>     global parameters 1
>   in third-party networks 1
> SNMP
>   retrieving information from network devices 1
> SRC ACP (SRC Admission Control Plug-In) 1
>   API 1
>   ATM access network 1
>   authorizing and tracking services 1
>   backbone network management, configuring 1
>   classification scripts
>     configuring 1
>   configuring 1
>   congestion points 1
>   connections to services directory, configuring 1
>   connections to subscribers’ directory, configuring 1
>   CORBA interfaces, configuring 1
>   data files 1
>   data files, reorganizing 1
>   description of 1
>   event publishers, configuring 1
>   external applications 1, 2
>   external plug-in for SAE, configuring 1
>   fault recovery 1
>   groups, configuring 1, 2
>   information from external applications, displaying 1
>   interactions with other components 1
>   logging properties, configuring 1
>   monitoring
>     C-Web interface 1
>     SRC CLI 1
>   operation, configuring 1
>   preventing service activation 1
>   properties 1
>   redundancy 1
>     configuring 1
>   SAE, configuring for 1
>   starting 1
>   state synchronization 1
>     configuring 1
>   stopping 1
>   subscribers, monitoring 1, 2
>   supporting multiple SAEs 1
>   using multiple SRC ACPs 1
> SRC ACP (SRC Admission Control Plug-In), congestion points 1
> SRC Admission Control Plug-In. See SRC ACP
> SRC client, JUNOSe routers
>   configuring 1
>   starting 1
>   stopping 1
> SRC software process, JUNOS routing platforms 1
>   disabling 1
>   reenabling 1
> starting
>   SRC ACP 1
> state synchronization
>   SRC ACP 1
> statistics, SRC ACP
>   monitoring
>     C-Web interface 1, 2, 3
> stopping SRC ACP 1
> subscribers
>   assigning interfaces to 1
>   configuring bandwidths and congestion points for 1, 2
>   IP addresses 1
>   login names 1
>   monitoring
>     C-Web interface 1, 2
>     SRC CLI 1, 2
>   provisioned and actual bandwidths 1
> subscriptions
>   reloading on SAE 1, 2
> support, technical See technical support

T

> targets. See classification scripts
> technical support
>   contacting JTAC 1
> text conventions defined 1
> third-party devices
>   creating sessions 1
>   integrating into SRC network
>     SRC CLI 1
>   logging in subscribers
>     assigned IP method 1
>     overview 1
>   provisioning with script services 1
>   router objects, adding
>     SRC CLI 1
>   SAE communities 1
>   VR objects, adding
>     SRC CLI 1
> threads
>   configuring for sessions
>     SRC CLI 1
> tracking plug-ins
>   virtual routers
>     SRC CLI 1, 2
> troubleshooting
>   JUNOS routing platforms 1
>   JUNOSe routers 1
> tuning factors for background bandwidth 1

U

> upstream bandwidth 1

V

> virtual routers
>   adding for third-party devices
>     SRC CLI 1
>   adding individually for JUNOSe routers
>     SRC CLI 1, 2
>   adding operative VRs 1
>     SRC CLI 1

[Contents] [Prev] [Next] [Index] [Report an Error]