> - Downloads
> - Configuring SRC ACP to Manage the Edge Network (C-Web Interface)
> - Related Topics
> - For more information about configuring residential subscribers, see Adding Subscribers (SRC CLI)
> - For more information about configuring services, see Adding a Normal Service (SRC CLI)
> - Configuring SRC-ACP to Manage the Backbone Network (C-Web Interface)
> - Viewing Information About Subscriber Sessions in the Edge Network (C-Web Interface)
> - Overview of SRC ACP

> # Configuring SRC ACP to Manage the Edge Network (C-Web Interface)

> To configure SRC ACP to manage the edge network, you must:

> 1. Configuring Network Interfaces in the Directory
> 2. Configuring Bandwidths for Subscribers (Edge Network)
> 3. Assigning Network Interfaces to Subscribers
> 4. Configuring Bandwidths for Services

> ## Configuring Network Interfaces in the Directory

> How you add network interfaces to the directory depends on the network type:

> - Edge networks—Specify the network interfaces of the routers and the switches in the access network between subscribers and the SRC network.
> - Backbone congestion points—Add only VRs and their interfaces.

> To configure the network interfaces of the routers and the switches in the access network:

> 1. Click Configure > Shared>Admission Control, expand the desired device.
> 2. If the device does not exist, from the Create new list, select Device. Type a name for the new device in the dialog box, and click OK.

>    The Device pane appears.

> 3. Enter information as described in the Help text in the main pane, and click Apply.

> ## Configuring Bandwidths for Subscribers (Edge Network)

> You must configure bandwidths for subscribers that SRC ACP manages in the edge region of the network.

> If congestion points cannot be derived from network access information, you must provide the following information for each subscriber.

> - Provisioned downstream bandwidth
> - Provisioned upstream bandwidth
> - Actual downstream bandwidth for the current subscriber session
> - Actual upstream bandwidth for the current subscriber session
> - List of DNs of interfaces associated with congestion points

> For further information, see SRC PE Network Guide.

> To configure bandwidths for subscribers:

> 1. Click Configure > Subscribers.
> 2. In the side pane, expand the desired retailer, expand the desired subscriber folder, and expand the desired subscriber.

>    The Admission Control pane appears.

> 3. Click Create, enter information as described in the Help text in the main pane, and click Apply.

> ## Assigning Network Interfaces to Subscribers

> You must assign to the subscriber object interfaces (including the router interfaces) for all congestion points between the subscriber and the router.

> | Note: You must define the interface in the directory before you can assign it to a residential subscriber (see Configuring Network Interfaces in the Directory ).

> To assign an interface:

> 1. Click Configure>Subscribers.
> 2. In the side pane, expand the desired retailer, and then click the desired subscriber folder.

>    The Admission Control pane appears.

> 3. Enter information in the Congestion Points box as described in the Help text in the main pane, and click Apply.

> ## Configuring Bandwidths for Services

> Upstream and downstream bandwidths must be specified for services that SRC ACP manages. You can obtain bandwidths for services in two ways:

> - Provide static values through the directory.
> - Allow the values to be provided through the SAE core API.

>   For example, a business partner may need to specify the required values for a particular piece of content through the SAE core API.

> To configure values for services:

> 1. For global configuration, click Configure>Services>Global and expand Service.
> 2. For scope configuration, click Configure>Services>Scope and expand Service.
> 3. In the side pane, expand the desired service and click Admission Control.

>    The Admission Control pane appears.

> 4. Click Create, enter information as described in the Help text in the main pane, and click Apply.

> #### Published: 2009-09-18

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.