> - Downloads
> - Configuring the SAE Community Manager with the C-Web Interface
> - Related Topics
> - For information about setting up SAE groups, see Configuring an SAE Group
> - Setting Up SAE Communities (C-Web Interface)
> - Configuring the SAE Community Manager
> - Using the SAE in a PCMM Environment

> # Configuring the SAE Community Manager with the C-Web Interface

> To configure the SAE community manager that manages PCMM device communities:

> 1. Click Configure, expand Shared>SAE, and then expand the SAE group for which you want to manage PCMM devices.
> 2. In the side pane, expand Configuration>External Interface Features: PCMMCommunityManager, and then click Community Manager.

>    The Community pane appears.

> 3. Enter information as described in the Help text in the main pane, and click Apply.

> #### Published: 2009-09-18

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.