[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring the SAE to Manage Network Devices (SRC CLI)

Use the following configuration statements to configure the device driver for MX Series routers:

`

shared sae configuration driver intelligent-service-edge {
  sae-community-manager sae-community-manager;
  cached-driver-expiration cached-driver-expiration;
  keep-alive-timeout keep-alive-timeout;
  registry-retry-interval registry-retry-interval;
  reply-timeout reply-timeout;
  sequential-message-timeout sequential-message-timeout;
  thread-pool-size thread-pool-size;
  thread-idle-timeout thread-idle-timeout;
}

`

To configure the device driver:

1. From configuration mode, access the statements for the device driver.
   `
   user@host# edit shared sae configuration driver intelligent-service-edge
   `
2. Specify the name of the community manager.
   `
   [edit shared sae configuration driver intelligent-service-edge]
   user@host# set sae-community-manager sae-community-manager
   `
3. (Optional) Specify the minimum amount of time to keep the state of a device driver after its Diameter connection is closed.
   `
   [edit shared sae configuration driver intelligent-service-edge]
   user@host# set cached-driver-expiration cached-driver-expiration
   `
4. (Optional) Specify the keepalive timeout before the registry to a Diameter server expires.
   `
   [edit shared sae configuration driver intelligent-service-edge]
   user@host# set keep-alive-timeout keep-alive-timeout
   `
5. (Optional) Specify the interval between retrying a failed registry to a Diameter server.
   `
   [edit shared sae configuration driver intelligent-service-edge]
   user@host# set registry-retry-interval registry-retry-interval
   `
6. (Optional) Specify the timeout before a request sent to a Diameter server expires.
   `
   [edit shared sae configuration driver intelligent-service-edge]
   user@host# set reply-timeout reply-timeout
   `
7. (Optional) Specify the timeout before an expected message expires.
   `
   [edit shared sae configuration driver intelligent-service-edge]
   user@host# set sequential-message-timeout sequential-message-timeout
   `
8. (Optional) Specify the number of working threads that process requests.
   `
   [edit shared sae configuration driver intelligent-service-edge]
   user@host# set thread-pool-size thread-pool-size
   `
9. (Optional) Specify the timeout for stopping working threads after they become idle.
   `
   [edit shared sae configuration driver intelligent-service-edge]
   user@host# set thread-idle-timeout thread-idle-timeout
   `
10. (Optional) Configure the session store parameters for the device driver.

    From configuration mode, access the statement that configures the session store for the device driver.

    `
    user@host# edit shared sae configuration driver intelligent-service-edge session-store
    `

    For more information about configuring session store parameters, see Configuring the Session Store Feature.

[Contents] [Prev] [Next] [Index] [Report an Error]