[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring JUNOS Routing Platforms to Interact with the SAE

To configure the JUNOS routing platform to interact with the SAE:

1. Include the following statements at the [edit system services service-deployment] hierarchy level.
   `
   [edit system services service-deployment]
   servers server-address {
     port port-number;
   }
   source-address source-address;
   `
2. Use the following guidelines for the variables in these statements.

- server-address —Specifies the IP address of the host on which you install the SAE. Be sure this setting matches the corresponding value in the SAE configuration.

- port-number— Specifies the port number for the SAE. Be sure this setting matches the corresponding value in the SAE configuration.

- source-address —(Optional) Specifies the IP address of the source that sends traffic to the SAE.

#### Related Topics

- Specifying Router Initialization Scripts on the SAE
- Configuring the JUNOS Routing Platform to Apply Changes It Receives from the SAE
- Disabling Interactions Between the SAE and JUNOS Routing Platforms
- Monitoring Interactions Between the SAE and JUNOS Routing Platforms

[Contents] [Prev] [Next] [Index] [Report an Error]