[Contents] [Prev] [Next] [Index] [Report an Error]

# Adding Network Devices (SRC CLI)

To set up the MX Series router so that it can be managed by the SAE:

1. From configuration mode, access the statements that configure network devices. You must specify the name of a device with lowercase characters. The name must match the Origin-Host AVP for the Diameter instance on the device. This sample procedure uses mx1 as the name of the router.
   `
   user@host# edit shared network device mx1
   `
2. Set the type of device to intelligent-service-edge.
   `
   [edit shared network device mx1]
   user@host# set device-type intelligent-service-edge
   `
3. Specify the configured peers associated with the device. See Configuring Diameter Peers (SRC CLI).
   `
   [edit shared network device mx1]
   user@host# set peers [peers...]
   `

   Note that MX Series routers support only a single peer connection.

4. From configuration mode, access the statements for virtual routers. The name must match the JSRC partition configured on the MX Series router, which is configured within the logical system:routing instance context. This sample procedure uses the name * for the virtual router.
   `
   [edit shared network device mx1]
   user@host# edit virtual-router *
   `

   where * matches any JSRC partition. You can also specify that the JSRC partition be configured in a logical system or in a logical system and routing instance. By default, logical system default and routing instance master are used.

5. Specify the SAEs that can manage this router.
   `
   [edit shared network device mx1 virtual-router default]
   user@host# set sae-connection [sae-connection...]
   `
6. (Optional) Verify your configuration.

       [edit shared network device mx1]
       user@host# show

[Contents] [Prev] [Next] [Index] [Report an Error]