> - Downloads
> - Specifying Initialization Scripts on the SAE
> - Related Topics
> - Specifying Initialization Scripts on the SAE
> - Setting Up Script Services
> - Copying Initialization Scripts to the C Series Controller
> - Developing Router Initialization Scripts for JUNOSe Routers, JUNOS Routing Platforms, and Network Devices

> # Specifying Initialization Scripts on the SAE

> Use the following configuration statements to specify initialization scripts for third-party devices:

> `
> shared sae configuration driver scripts {
>   extension-path extension-path ;
>   general general ;
> }
> `

> To configure initialization scripts for third-party devices:

> 1. From configuration mode, access the configuration statements that configure initialization scripts.
>    `
>    user@host# edit shared sae configuration driver scripts
>    `
> 2. Specify the initialization script for third-party devices.
>    `
>    [edit shared sae configuration driver scripts]
>    user@host# set general general
>    `
> 3. Configure a path to scripts that are not in the default location, /opt/UMC/sae/lib.
>    `
>    [edit shared sae configuration driver scripts]
>    user@host# set extension-path extension-path
>    `
> 4. (Optional) Verify your initialization script configuration.

>        [edit shared sae configuration driver scripts]
>        user@host# show

> #### Published: 2009-09-15

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.