> - Downloads
> - Configuring the SAE to Use TLS
> - Related Topics
> - Configuring the SAE to Manage JUNOS Routing Platforms (C-Web Interface)
> - Configuring TLS on the SAE
> - Configuring JUNOS Routing Platforms to Interact with the SAE
> - Monitoring Interactions Between the SAE and JUNOS Routing Platforms

> # Configuring the SAE to Use TLS

> To configure the SAE to accept TLS connections:

> 1. Click Configure, expand Shared>Network, and then click a JUNOS router.

>    The Device pane appears.

> 2. Type a port number in the Beep Server Port box, and click Apply.

> #### Published: 2009-09-18

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.