[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring TLS on the SAE

To configure TLS on the SAE:

1. Click Configure, expand Shared>SAE>Configuration>Driver>JUNOS, and then click Security.

   The Security pane appears.

2. Click Create, enter information as described in the Help text in the main pane, and then click Apply.

#### Related Topics

- Configuring the SAE to Use TLS
- Configuring the SAE to Manage JUNOS Routing Platforms (C-Web Interface)
- Monitoring Interactions Between the SAE and JUNOS Routing Platforms

[Contents] [Prev] [Next] [Index] [Report an Error]