[Contents] [Prev] [Next] [Index] [Report an Error]

## Example: Managing Specific Interfaces

This example causes the SAE to load the DHCP policy group on IP interfaces on Fast Ethernet modules in slot 3/port 1, slot 1/port 1, or any port on slot 2. The SAE then manages these interfaces.

    [edit shared network device erx-node2 interface-classifier rule rule-1]
    user@host# show
    target /junose/DHCP;
    condition {
      interfaceName=FastEthernet3/1;
      interfaceName=FastEthernet1/1;
      interfaceName=FastEthernet2/*;
    }

#### Related Topics

- Overview of Configuring Classification Scripts
- Overview of Classification Scripts
- Sending DHCP Options to the JUNOSe Router
- DHCP Options Supported on the SAE

[Contents] [Prev] [Next] [Index] [Report an Error]