> - Downloads
> - Viewing Statistics for Specific JUNOSe Device Drivers (SRC CLI)
> - Related Topics
> - Troubleshooting Problems with Managing JUNOSe Routers
> - Viewing Statistics for All JUNOSe Device Drivers (SRC CLI)
> - Monitoring Interactions Between the SAE and the JUNOSe Router
> - Viewing the State of JUNOSe Device Drivers (C-Web Interface)

> # Viewing Statistics for Specific JUNOSe Device Drivers (SRC CLI)

> #### Purpose

> Display statistics for a specific JUNOSe device driver.

> #### Action

> Use the following operational mode command:

> `
> show sae statistics device <name name> < (brief) >
> `

> For example:

> `user@host> show sae statistics device name default@dryad`

>     SNMP Statistics
>     Add notification handle time       6
>     Change notification handle time    0
>     Client ID                          default@dryad
>     Delete notification handle time    0
>     Failover IP                        0.0.0.0
>     Failover port                      0
>     Handle message time                60
>     Job queue age                      0
>     Job queue time                     4
>     Number message send                158
>     Number of added jobs               9
>     Number of add notifications        4
>     Number of change notifications     0
>     Number of delele notifications     0
>     Number of managed interfaces       4
>     Number of message errors           0
>     Number of message timeouts         0
>     Number of removed jobs             9
>     Number of user session established 0
>     Number of user session removed     0
>     Router type                        JUNOSE COPS
>     Up time                            172286
>     Using failover server              false

> #### Published: 2009-09-15

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.