[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring Fixed Public Addresses for Outgoing Traffic

To configure fixed public IP addresses for outgoing traffic:

1. Set the portal configuration level to Advanced (see Setting the Configuration Level for Enterprise Manager Portal).
2. Locate the area called Fixed Public Addresses for Outgoing Traffic in the NAT page (see Figure 27).
3. Click Create.

[Contents] [Prev] [Next] [Index] [Report an Error]