[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring the Remote Diameter Peer (SRC CLI)

Use the following configuration statements to configure the remote Diameter peer:

`

slot number ims aracf-rq peer name {
  address address;
  port port;
  origin-host origin-host;
  watchdog-timeout watchdog-timeout;
  incoming-queue-limit incoming-queue-limit;
}

`

To configure the remote Diameter peer:

1. From configuration mode, access the statement that configures the Diameter peer. In this sample procedure, the remote SPDF peer called primary-spdf is configured.
   `
   user@host# edit slot 0 ims aracf-rq peer primary-spdf
   `
2. (Optional) Specify the IP address of the remote peer.
   `
   [edit slot 0 ims aracf-rq peer primary-spdf]
   user@host# set address address
   `
3. (Optional) Specify the port of the remote peer.
   `
   [edit slot 0 ims aracf-rq peer primary-spdf]
   user@host# set port port
   `
4. (Optional) Specify the Diameter identifier for the remote endpoint that is the originator of the Diameter message.
   `
   [edit slot 0 ims aracf-rq peer primary-spdf]
   user@host# set origin-host origin-host
   `
5. (Optional) Specify the watchdog timeout of the connection to the remote peer.
   `
   [edit slot 0 ims aracf-rq peer primary-spdf]
   user@host# set watchdog-timeout watchdog-timeout
   `
6. (Optional) Specify the size of the incoming message queue before the system rejects messages.
   `
   [edit slot 0 ims aracf-rq peer primary-spdf]
   user@host# set incoming-queue-limit incoming-queue-limit
   `
7. (Optional) Verify your configuration.

       [edit slot 0 ims aracf-rq peer primary-spdf]
       user@host# show
       address 127.0.0.1;
       origin-host testclient;

#### Related Topics

- Overview of an IMS Environment
- Configuring the IMS Software (SRC CLI)
- Configuring the Local Diameter Peer (SRC CLI)
- Monitoring IMS (SRC CLI)

[Contents] [Prev] [Next] [Index] [Report an Error]