> - Downloads
> - Modifying the JPS Configuration (C-Web Interface)
> - Related Topics
> - Modifying the JPS Configuration
> - Configuring the JPS (C-Web Interface)
> - Modifying the Subscriber Configuration (C-Web Interface)
> - Overview of the JPS

> # Modifying the JPS Configuration (C-Web Interface)

> Tasks to modify the current JPS configuration are:

> 1. Configuring General Properties for the JPS (C-Web Interface)
> 2. Specifying a Policy Server Identifier in Messages (C-Web Interface)
> 3. Configuring Logging Destinations (C-Web Interface)
> 4. Specifying Connections to the Application Managers (C-Web Interface)
> 5. Specifying Connections to RKSs (C-Web Interface)

> ## Configuring General Properties for the JPS (C-Web Interface)

> To configure general properties for the JPS:

> 1. Click Configure, and expand Slot>Slot: 0, and then click JPS.

>    The JPS pane appears.

> 2. Enter the information in the main pane as described in the Help text, and click Apply.

> ## Specifying a Policy Server Identifier in Messages (C-Web Interface)

> To configure a policy server identifier for the JPS:

> 1. Click Configure, expand Slot>Slot: 0, and then click JPS.

>    The JPS pane appears.

> 2. In the Policy Server ID box, enter a value as described in the Help text in the main pane.
> 3. Enter information in the remaining boxes as described in the Help text in the main pane, and click Apply.

> ## Configuring Logging Destinations (C-Web Interface)

> You can configure the logging destination to store messages in a file, or to a system logging facility (Syslog)

> You can create or modify loggers. By default, the JPS has four logging destinations (log1, log2, log3, and log4).

> ## Specifying Connections to the Application Managers (C-Web Interface)

> This section describes how to configure the application manager–to–policy server interface (PKT-MM3) so that the policy server can communicate with application managers.

> To configure the connections to the application managers:

> 1. Click Configure, expand Slot>Slot: 0>JPS, and then click AM Interface.

>    The AM Interface pane appears.

> 2. Enter the information in the main pane as described in the Help text, and click Apply.

> ## Specifying Connections to RKSs (C-Web Interface)

> To configure the policy server–to–RKS interface (PKT-MM4) so that policy events can be sent to the RKS, you can configure RKS pairs and their associated application managers.

> To configure the policy server–to–RKS interface:

> 1. Click Configure, expand Slot>Slot: 0>JPS, and then click RKS Interface.

>    The RKS Interface pane appears.

> 2. Enter the information in the main pane as described in the Help text, and click Apply.

> #### Published: 2009-09-18

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.