[Contents] [Prev] [Next] [Index] [Report an Error]

# Viewing Information About Boot Messages (SRC CLI)

#### Purpose

If you encounter system problems in a C Series Controller after you start the system, you can view information about the boot process.

View messages generated during system boot.

#### Action

`user@host> show system boot-messages`

    Bootdata ok (command line is ro root=/dev/vg0/root console=tty0 console=ttyS0,96
    00)
    Linux version 2.6.9-42.0.3.ELsmp (buildcentos@x8664-build.centos.org) (gcc versi
    on 3.4.6 20060404 (Red Hat 3.4.6-3)) #1 SMP Fri Oct 6 06:28:26 CDT 2006
    BIOS-provided physical RAM map:
     BIOS-e820: 0000000000000000 - 000000000009ac00 (usable)
     BIOS-e820: 000000000009ac00 - 00000000000a0000 (reserved)
     BIOS-e820: 00000000000ea070 - 0000000000100000 (reserved)
     BIOS-e820: 0000000000100000 - 00000000dffc0000 (usable)
     BIOS-e820: 00000000dffc0000 - 00000000dffcf000 (ACPI data)
     BIOS-e820: 00000000dffcf000 - 00000000dfff0000 (ACPI NVS)
     BIOS-e820: 00000000dfff0000 - 00000000e0000000 (reserved)
     BIOS-e820: 00000000fec00000 - 00000000fec86000 (reserved)
     BIOS-e820: 00000000fee00000 - 00000000fee01000 (reserved)
     BIOS-e820: 00000000ffb00000 - 0000000100000000 (reserved)
     BIOS-e820: 0000000100000000 - 0000000220000000 (usable)
    ACPI: RSDP (v000 ACPIAM                                ) @ 0x00000000000f7760
    ACPI: RSDT (v001 A M I  OEMRSDT  0x03000529 MSFT 0x00000097) @ 0x00000000dffc000
    0
    ACPI: FADT (v002 A M I  OEMFACP  0x03000529 MSFT 0x00000097) @ 0x00000000dffc020
    0
    ACPI: MADT (v001 A M I  OEMAPIC  0x03000529 MSFT 0x00000097) @ 0x00000000dffc039
    0
    ACPI: OEMB (v001 A M I  AMI_OEM  0x03000529 MSFT 0x00000097) @ 0x00000000dffcf04
    0
    ACPI: DSDT (v001  DVLG2 DVLG2007 0x00000007 INTL 0x02002026) @ 0x000000000000000
    0
    No NUMA configuration found
    Faking a node at 0000000000000000-0000000220000000
    Bootmem setup node 0 0000000000000000-0000000220000000
    No mptable found.
    On node 0 totalpages: 2228224
      DMA zone: 4096 pages, LIFO batch:1
      Normal zone: 2224128 pages, LIFO batch:16
      HighMem zone: 0 pages, LIFO batch:1
    DMI 2.3 present.
    ACPI: PM-Timer IO Port: 0x408
    ACPI: Local APIC address 0xfee00000
    ACPI: LAPIC (acpi_id[0x01] lapic_id[0x00] enabled)
    Processor #0 15:4 APIC version 16
    ACPI: LAPIC (acpi_id[0x02] lapic_id[0x06] enabled)
    Processor #6 15:4 APIC version 16
    ACPI: LAPIC (acpi_id[0x03] lapic_id[0x01] enabled)
    Processor #1 15:4 APIC version 16
    ACPI: LAPIC (acpi_id[0x04] lapic_id[0x07] enabled)
    Processor #7 15:4 APIC version 16
    Setting APIC routing to flat
    ACPI: IOAPIC (id[0x08] address[0xfec00000] gsi_base[0])
    IOAPIC[0]: apic_id 8, version 32, address 0xfec00000, GSI 0-23
    ACPI: IOAPIC (id[0x09] address[0xfec10000] gsi_base[24])
    IOAPIC[1]: apic_id 9, version 32, address 0xfec10000, GSI 24-4
    ACPI: INT_SRC_OVR (bus 0 bus_irq 0 global_irq 2 dfl dfl)
    ACPI: INT_SRC_OVR (bus 0 bus_irq 9 global_irq 9 high level)
    ACPI: IRQ0 used by override.
    ACPI: IRQ2 used by override.
    ACPI: IRQ9 used by override.
    Using ACPI (MADT) for SMP configuration information
    Allocating PCI resources starting at e2000000 (gap: e0000000:1ec00000)
    Checking aperture...
    Built 1 zonelists
    Kernel command line: ro root=/dev/vg0/root console=tty0 console=ttyS0,9600
    Initializing CPU#0
    PID hash table entries: 4096 (order: 12, 131072 bytes)
    time.c: Using 3.579545 MHz PM timer.
    time.c: Detected 3200.267 MHz processor.
    Console: colour VGA+ 80x25
    Dentry cache hash table entries: 2097152 (order: 12, 16777216 bytes)
    Inode-cache hash table entries: 1048576 (order: 11, 8388608 bytes)
    Placing software IO TLB between 0x28c1000 - 0x68c1000
    Memory: 8168568k/8912896k available (2106k kernel code, 0k reserved, 1297k data,
     196k init)
    Calibrating delay using timer specific routine.. 6406.43 BogoMIPS (lpj=3203218)
    Security Scaffold v1.0.0 initialized
    SELinux:  Initializing.
    SELinux:  Starting in permissive mode
    There is already a security framework initialized, register_security failed.
    selinux_register_security:  Registering secondary module capability
    Capability LSM initialized as secondary
    Mount-cache hash table entries: 256 (order: 0, 4096 bytes)
    CPU: Trace cache: 12K uops, L1 D cache: 16K
    CPU: L2 cache: 2048K
    using mwait in idle threads.
    CPU0: Initial APIC ID: 0, Physical Processor ID: 0
    Using IO APIC NMI watchdog
    CPU: Trace cache: 12K uops, L1 D cache: 16K
    CPU: L2 cache: 2048K
    CPU0: Initial APIC ID: 0, Physical Processor ID: 0
    CPU0:                   Intel(R) Xeon(TM) CPU 3.20GHz stepping 03
    per-CPU timeslice cutoff: 705.82 usecs.
    task migration cache decay timeout: 1 msecs.
    Booting processor 1/6 rip 6000 rsp 10006945f58
    Initializing CPU#1
    Calibrating delay using timer specific routine.. 6399.38 BogoMIPS (lpj=3199690)
    CPU: Trace cache: 12K uops, L1 D cache: 16K
    CPU: L2 cache: 2048K
    CPU1: Initial APIC ID: 6, Physical Processor ID: 3
                      Intel(R) Xeon(TM) CPU 3.20GHz stepping 03
    Booting processor 2/1 rip 6000 rsp 1000697df58
    Initializing CPU#2
    Calibrating delay using timer specific routine.. 6399.32 BogoMIPS (lpj=3199664)
    CPU: Trace cache: 12K uops, L1 D cache: 16K
    CPU: L2 cache: 2048K

#### Related Topics

- Viewing Information About Boot Messages (C-Web Interface)
- Viewing Information About a C Series Controller
- Viewing Information About Components Installed (SRC CLI)
- Viewing Information About System Disk Status
- For information about configuring C Series Controllers, see the SRC PE C-Web Interface Configuration Guide

[Contents] [Prev] [Next] [Index] [Report an Error]