> - Downloads
> - Configuring External Subscriber Monitor (C-Web Interface)

> # Configuring External Subscriber Monitor (C-Web Interface)

> Configure initial properties, including directory connection and directory eventing properties.

> Tasks to configure External Subscriber Monitor are:

> 1. Configuring Basic Local Properties for External Subscriber Monitor
> 2. Configuring Initial Properties for External Subscriber Monitor
> 3. Configuring Directory Connection Properties for External Subscriber Monitor
> 4. Configuring Eventing Properties for External Subscriber Monitor
> 5. Configuring Logging Destinations for External Subscriber Monitor

> ## Configuring Basic Local Properties for External Subscriber Monitor

> To configure basic local properties:

> 1. Click Configure>Slot, then a specified slot (for example, slot0), and then External Subscriber Monitor.

>    The External Subscriber Monitor pane appears.

> 2. From the Create new list, select Logger. Type a name for the new logger in the dialog box, and click OK.
> 3. Enter the maximum java heap size in the Java Heap Size box, as described in the Help text.
> 4. Click Apply.

> ## Configuring Initial Properties for External Subscriber Monitor

> To configure initial properties:

> 1. Click Configure>Slot, then a specified slot (for example, slot0).
> 2. Expand External Subscriber Monitor.
> 3. Click Initial.

>    The Initial pane appears.

> ## Configuring Directory Connection Properties for External Subscriber Monitor

> To configure directory connection properties:

> 1. Click Configure>Slot, then a specified slot (for example, slot0).
> 2. Expand External Subscriber Monitor.
> 3. Expand Initialand, then click Directory Connection.

>    The Directory Connection pane appears.

> 4. Enter the information as described in the Help text box.
> 5. Click Apply.

> ## Configuring Eventing Properties for External Subscriber Monitor

> To configure eventing properties:

> 1. Click Configure>Slot, then a specified slot (for example, slot0).
> 2. Expand External Subscriber Monitor.
> 3. Expand Initial, and then click Directory Eventing.

>    The Directory Eventing pane appears.

> 4. Enter the information as described in the Help text box.
> 5. Click Apply.

> ## Configuring Logging Destinations for External Subscriber Monitor

> You can configure the logging destination to store messages in a file or a system logging facility (Syslog). You can create or modify loggers.

> To configure logging destinations to store log messages:

> 1. Click Configure>Slot, then a specified slot (for example, slot0).
> 2. Expand External Subscriber Monitor.
> 3. From the Create new list, select Logger.
> 4. In the dialog box, type a name for the new logger, and click OK.

>    The name of the logger appears in the side pane and the Logger pane.

> 5. Expand the logger in the side pane, and then click File or Syslog.
> 6. Click Create, enter information as described in the Help text in the main pane, and click Apply.

> #### Published: 2009-09-18

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.