[Contents] [Prev] [Next] [Index] [Report an Error]

## Example: Configuring JUNOSe Policies for IMS (SRC CLI)

For IMS environments, you can configure JUNOSe policies. When you configure classify-traffic conditions, you can set up the software so that the SAE expands into multiple classifiers before it installs the policy on the router. If you enter a list of values in the source and destination network (IP address, mask, and IP operation) or port fields (for port-related protocols), the software creates a classifier for each possible combination of address and port. Note that the software does not expand classifiers for values that are entered as a range.

## Enabling Expansion of JUNOSe Classify-Traffic Conditions

To enable the expansion of JUNOSe classify-traffic conditions:

1. From configuration mode, access the statement that configures policy management properties on the SAE.
   `
   user@host# edit shared sae configuration policy-management-configuration
   `
2. Specify whether or not the SAE expands the JUNOSe classify-traffic conditions into multiple classifiers before it installs the policy on the router.
   `
   [edit shared sae configuration policy-management-configuration]
   user@host# set enable-junose-classifier-expansion
   `

#### Related Topics

- For more information about expanded classifiers, see Policy Information Model
- Configuring Classify-Traffic Conditions
- Policy Management Overview

[Contents] [Prev] [Next] [Index] [Report an Error]