> - Downloads
> - Configuring the JPS (C-Web Interface)
> - Related Topics
> - Configuring the JPS
> - Starting the JPS (C-Web Interface)
> - Displaying JPS Status (C-Web Interface)
> - For information about monitoring the JPS with the C-Web interface, see the SRC PE Solutions Guide
> - Overview of the JPS

> # Configuring the JPS (C-Web Interface)

> You can modify the JPS configuration, which includes configuring the logging destinations and connections to the JPS interfaces. Any configuration changes will be applied within 15 seconds.

> You can configure the subscriber, which maps a subscriber address to the CMTS address.

> The tasks to configure the JPS for a cable network environment are:

> 1. Modifying the JPS Configuration (C-Web Interface)
> 2. Modifying the Subscriber Configuration (C-Web Interface)

> In addition to configuring the JPS, you might need to perform these tasks:

> 1. Configuring the SAE to Interact with the JPS (C-Web Interface)
> 2. Using the NIC Resolver in PCMM Environments .

> #### Published: 2009-09-18

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.