[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring IPMI with the C-Web Interface

For the C2000 model, an IPMI configuration includes an IP address assigned to the IPMI interface and a gateway IP address. For the C4000 model, only a gateway IP address is required because the IP address for the IPMI interface is the same as the IP address assigned to the eth0 interface on the C4000 model.

To configure IPMI on an interface:

1. Click Configure, expand System, and then click IPMI.

   The IPMI pane appears.

2. In the Address box, enter an IP address.
   - An IP address is required for a C2000 model but is set automatically to the address of the eth0 interface on a C4000 model.
   - address is in the format IP address/destination prefix, such as 10.227.7.145/24.

3. In the Gateway box, enter the default gateway IP address.

   A default gateway is a node on a network that serves as an access point to another network.

4. Click Apply.

   The IPMI pane displays the new attributes.

[Contents] [Prev] [Next] [Index] [Report an Error]