[Contents] [Prev] [Next] [Index] [Report an Error]

# Configuring QoS Profile Attachment Actions (C-Web Interface)

Use this action to specify the name of the QoS profile to attach to the router interface when this action is taken. You can configure QoS actions for JUNOSe policy rules.

The router allows only one QoS profile to be attached to an interface at one time. Therefore, as a subscriber activates and deactivates different services, the QoS profile running on the interface needs to change. The SRC module provides a QoS-tracking plug-in (QTP) that you can use to ensure that as a subscriber activates and deactivates services, the required QoS profile is attached to the subscriber interface. See Dynamically Managing QoS Profiles .

To configure a QoS profile attachment action:

1. In the side pane, select a JUNOSe policy rule.
2. From the Create new list, select Qos Attach. Type a name for the QoS profile attachment action, and click OK.
3. Enter information as described in the Help text in the main pane, and click Apply.

#### Related Topics

- Delivering QoS Services in a Cable Environment
- Configuring QoS Profile Attachment Actions (SRC CLI)
- Configuring QoS Conditions with the C-Web Interface

[Contents] [Prev] [Next] [Index] [Report an Error]