> - Downloads
> - Adding a Mutex Group (C-Web Interface)
> - Related Topics
> - SRC PE Services and Policies Guide

> # Adding a Mutex Group (C-Web Interface)

> You can add a mutex group in the global service scope or in a service scope.

> To add a mutex group:

> 1. Click Configure, and expand Services.
> 2. To add a mutex group in the global service scope:
>    1. Click Global.
>    2. From the Create new list, select Mutex Group.
>    3. Type a name for the new mutex group in the dialog box, and click OK.
> 3. To add a mutex group in the service scope:
>    1. Click the specified scope.
>    2. From the Create new list, select Mutex Group.
>    3. Type a name for the new mutex group in the dialog box, and click OK.
> 4. The Mutex Group: <name> pane appears.
> 5. Enter information as described in the Help text in the main pane, and click Apply.

> #### Published: 2009-09-18

> Copyright © 2009, Juniper Networks, Inc. All rights reserved. Trademark Notice.