Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

# Setting the Logging Level (CTPView Server Menu)

You can specify the logging level, which determines what events are logged The log output is placed in the /var/log/acorngui.log file.

Before you begin, log in to the CTPView server and access the CTPView Configuration Menu. See Accessing the CTPView Server Configuration Menu (CTPView Server Menu).

To set the logging level:

1. From the CTPView Configuration Menu, select 4) Advanced Functions.
2. Select 7) Set Logging Level.

3. Enter one of the following:

   - 1) Normal (Most commands, All errors)
   - 2) Debug Level 1 (All commands, All errors)
   - 3) Debug Level 2 (All commands, All output)

#### Published: 2010-10-05

﻿
Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out