Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

# Configuring Bundle Pairs for TDM/TDC Operation (CTP Menu)

The TDM/TDC feature is supported on CTP2000 serial interfaces. TDM/TDC operation requires both a low-speed bundle and a high-speed bundle. This topic describes how to configure the high-speed and low-speed bundle port options when used for TDM/TDC bundles using CTP Menu.

1. Configuring the High-Speed CTP Bundle for TDM/TDC Operation (CTP Menu)
2. Configuring the Low-Speed CTP Bundle for TDM/TDC Operation (CTP Menu)

## Configuring the High-Speed CTP Bundle for TDM/TDC Operation (CTP Menu)

Configure the high-speed bundle on an even-numbered port.

Before you begin:

- Disable the bundle before you modify the bundle options.

To configure a high-speed CTP bundle for TDM/TDC operation using the CTP Menu:

1. From the Main Menu, select 1) Bundle Operations.
2. Select 1) CTP.
3. Select a bundle from the list. You must configure the bundle on an even-numbered port.

   If you select an active bundle, you are prompted to disable the bundle before configuring it.

4. Select 3) Port Config.
5. Select 2) Interface.
6. Select 3) Encoding.
7. Select 5) TDM.
8. Follow the onscreen instructions to configure the parameters in Table 1.
9. Configure the rest of the bundle as you normally would.

Table 1: High-Speed CTP Bundle Parameters for TDM/TDC Operation in the CTP Menu

Field | Function | Your Action
--- | --- | ---
TDC Clk/Data on port N+1 | Specifies that the TDM function is TDC Clk/Data on port N+1. This option is available only on even numbered ports on a CTP2000 serial module, and when the serial encoding parameter is set to TDM. TDC Clk/Data on port N+1 oversamples the incoming clock (TT) and data (SD) from the adjacent port above this one (N+1) at this port’s clock rate, and embeds it in its data. At the remote end of the network, the embedded circuit data is recovered and exits the node on port N+1 as RT and RD outputs. Because of the direct interleaving of two ports’ data, TDC is maintained between these two ports with an accuracy of one bit time at this port’s data rate. | Press Enter.
TDM rates | Specifies the number of bits out of 32 that are used for the TDM function (and not for local serial port data). Appears only if you selected TDM encoding. Keep in mind the following when you configure the TDM rate: If the rate is too low, the bundle may not carry the low-speed data because of insufficient oversampling. If the rate is too high, the low-speed circuit will still run, but will likely use more bandwidth than necessary. You may want to configure a higher rate to increase the TDM rate to reduce jitter on the low-speed clock and data signals. | Select one: 16 8 4 2

## Configuring the Low-Speed CTP Bundle for TDM/TDC Operation (CTP Menu)

Configure the low-speed bundle on an odd-numbered port that is one higher than the corresponding high-speed bundle.

Before you begin:

- Disable the bundle before you modify the bundle options.

To configure the low-speed CTP bundle using CTP Menu:

1. From the Main Menu, select 1) Bundle Operations.
2. Select 1) CTP.
3. Select a bundle from the list. The bundle must be configured on an even-numbered port.

   If you select an active bundle, you are prompted to disable the bundle before configuring it.

4. Select 3) Port Config.
5. Select 3) Clock Config.
6. Select 1) Port Clock Config.
7. Select 8) TDM/TDC - Interleaved Slow Port.

| Note: Do not configure any other bundle parameters.

#### Published: 2011-01-09

﻿
Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out