Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

# Allocating Channels for Analog Interfaces for VComp Bundles (CTP Menu)

This topic describes how to allocate channels for VComp bundles.

You can configure up to 30 voice channels on a VComp bundle. These channels can be one type only. For example, if the first channel of a VComp bundle is a 4WE&M type; any additional channels added to the bundle must be of the same type.

Before you begin:

- Disable the bundle before you modify the bundle options.

To allocate channels using the CTP Menu:

1. From the Main Menu, select 1) Bundle Operations.
2. Select 4) VCOMP.
3. Select a bundle from the list.

   If you select an active bundle, you are prompted to disable the bundle before configuring it.

4. Select 2) Config.
5. Select 3) Channel Allocation.
6. Follow the onscreen instructions, and configure the option as described in Table 1.

Table 1: VComp Bundle Channel Allocation Parameter Settings in the CTP Menu

Field | Function | Your Action
--- | --- | ---
Channel Allocation (for analog interfaces) | Adds interfaces to or removes interfaces from the bundle. It is important to note that the order of the channels (indicated by the XX: prefix on the channel allocation display) corresponds to the relative channel positions of the channels in the bundle. They connect on a one-to-one basis with the channels in the VComp bundle on the remote end of the network. When channels are removed from a VComp bundle, remaining channels are shifted left. | Select one: 1) remove—Enter the port that you want to remove. 2) add—Enter the port that you want to add.

#### Published: 2010-10-27

﻿
Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out