Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

## Related Documentation

- Enabling Ethernet Interface Failover (CTPView)

# Ethernet Interface Failover Overview

When the CTP device sends traffic over the IP network, it aggregates the traffic over its Ethernet interfaces. When you configure your Ethernet interfaces, you specify which Ethernet interface is the default Ethernet interface. In the AutoSwitch configuration, you can enable failover on the default Ethernet interface. If the default Ethernet interface goes down, the CTP device switches to the next unconfigured Ethernet interface.

## Related Documentation

- Enabling Ethernet Interface Failover (CTPView)

#### Published: 2010-10-26

﻿
Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out