Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

# Displaying Running VComp Bundle Configuration and Counters (CTP Menu)

To display a bundle using the CTP Menu:

1. From the Main Menu, select 1) Bundle Operations.
2. Select 4) VCOMP.
3. Select a bundle from the list.
4. Select 1) Query.

Table 1: VComp Bundle Runtime State Counters in the CTP Menu

Field Name | Field Description
--- | ---
Runtime State | ACTIVE or DISABLED
DSP Info(dsp/bndl) | Indicates which voice compression module (DSP) the bundle is built on, as well as the bundle allocation ID on the voice compression module.
Voice Channel Signaling | Current voice signaling. This field is displayed for VComp bundles that carry analog voice interfaces as well as VComp bundles that transport T1/E1 ports with signaling enabled. This information is not displayed for VComp bundles transporting channels from T1/E1 interfaces with signaling disabled. Under Chan Src, the XX: prefix indicates the channel number.
T1E1 flags | Current T1 or E1 flag: LOS—Loss of signal LOF—Loss of frame
I/F bound packets | Number of packets received from the IP network destined for the bundle.
NET bound packets | Number of packets created by the bundle and sent to the IP network.
Missing pkts | Number of packets destined for the bundle that were not available at the time when that data was needed. This unavailability may be due to a dropped packet in the IP network or to a packet that arrived too late at the CTP device to be processed out the interface. Both dropped and late packets cause the missing packet counter to increment.
Buffer underflows | Number of times the buffer reached the minimum set threshold.
Buffer overflows | Number of times the buffer reached the maximum set threshold.
Buffer starves | Indicates an exceeded threshold. The CTP device is designed to tolerate strings of consecutive missing packets without the loss of bit count integrity. The number of packets is configurable; the default is five (5). Exceeding this threshold is called a starvation, and a counter is incremented each time this event occurs.
Buffer average | Average buffer size in ms.

#### Published: 2010-10-27

﻿
Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out