Country

- China
- France
- Germany
- Japan
- Korea
- Spain
- Taiwan
- United Kingdom
- United States

Contact Us
|
Country
United States

# Technical Documentation

- Download Software
- Research a Problem
- Case Management
- Contract & Product Management
- Technical Documentation
  - Advanced Search
  - Documentation Archive
  - Documentation Bug Report
  - Enterprise MIBs
  - File Format Help
  - Glossary
  - Portable Libraries
- End-of-Life Products
- Contact Support
- Guidelines and Policies
- Security Resources

- Downloads
- CTP2000 Compression Interface Module

- Related Topics
- CTP2000 Series Serial Interface Modules
- CTP2000 Series T1/E1 Interface Module
- CTP2000 4W&EM Interface Module CTP2000 4W&EM Interface Module
- CTP2000 2W-FXS and 2W-FXO Interface Modules
- CTP2000 8P-IRIG Interface Module

# CTP2000 Compression Interface Module

The CTP2000 Series compression interface module enables serial data and voice bundles to be compressed and passed through a CTP2000 platform. (See Figure 1.)

Voice bundles originating from the CTP2000 IM-8P-T1/E1, analog CTP2000 IM-4WE&M, IM-2WFXS, and IM-2WFXO modules use the CTP2000 compression module to compress the voice bundle. Voice bundles ranging from 1–24 channels on a T1 module, 1–30 channels on an E1 module, and 1–8 channels on a 4WE&M module can be bundled and connected through the compression module to compress the voice bundle and build the IP packet.

Figure 1: Compression Interface Module

The compression module supports these compression algorithms:

- MELP (2.4k)
- G.729AB (8k)
- G.728 (16k)
- G.726 (16k)
- G.726 (32k)
- PMC (64k)

The module supports Mu-Law and A-Law companding, echo cancellation, silence suppression, fax/modem detection, and tone relay. You can configure the compression options when configuring the voice bundle.

#### Published: 2010-05-11