Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

## Related Documentation

- Installing a CTP Interface Module, Processor Module, or Clock Module

# Installing or Removing a CTP150 CompactFlash Card

The CompactFlash card is installed in the rear panel of the CTP150. To remove or install the CompactFlash card:

1. Power off the unit.
2. Remove the CompactFlash face plate in the center of the rear panel by unscrewing the two retaining screws.
3. Remove or install the CompactFlash card in the flash socket.
4. Replace the face plate with the two retaining screws.

## Related Documentation

- Installing a CTP Interface Module, Processor Module, or Clock Module

#### Published: 2011-01-31

﻿
Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out