Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

## Related Documentation

- CESoPSN Bundle Overview
- Configuring IP Parameters for CESoPSN Bundles on CTP2000 Devices (CTPView)

# Configuring DS0 Time Slots for CESoPSN Bundles (CTPView)

This topic describes how to configure the DS0 time slots used by the bundle. By default, all unused DS0s are attached to a bundle. An unused DS0 is a DS0 not assigned to another bundle.

Before you begin:

- Log in to the CTPView software at least at the Net_Admin level.
- Connect the CTPView server to the CTP device for which you want to configure bundles.
- Disable the bundle before you modify the bundle options.

To configure time slots for CESoPSN bundles using CTPView:

1. In the side pane, select Bundle > Configuration.
2. Run your mouse over the Display and Select an Existing Bundle bar.
3. In the table of bundles, select the bundle that you want to modify.
4. Under Bundle Options, configure the parameters described in Table 1, and click Click to Submit Bundle AND Port Changes.

Table 1: CESoPSN Bundle DS0 Time Slot Settings in CTPView

Field | Function | Your Action
--- | --- | ---
Time Slots [ Selected are green. ] | Specifies the time slots that are assigned to the bundle. The number of time slots that you select affects the default packet size and packet buffer set size for the bundle. | Click on a time slot to select it for the bundle. Green time slots are selected. Gray time slots are not selected.

## Related Documentation

- CESoPSN Bundle Overview
- Configuring IP Parameters for CESoPSN Bundles on CTP2000 Devices (CTPView)

#### Published: 2010-10-26

﻿
Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out