Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

## Related Documentation

- Setting Up Management Access on the CTP2000 Platform
- CTP2000 Console Port Setup
- Using HyperTerminal with the CTP2000 Platform
- CTP2000 Platform SSH Setup

# Connecting Directly to the CTP2000 Platform

When you connect a console directly to the device, use the COM 2 port on the RJ-45 connector. To do this, you must use the special DB-9 adapter with a straight-through RJ-45 cable. Direct access through the COM 2 serial port enables you to monitor the device while it boots.

To connect a console directly to the device:

1. Connect the female DB-9 connector to the COM 2 port on the device’s RTM.
2. Connect the crossover adapter connector to your PC's serial port.
3. Power on the device.

   When you power on the device, the CLI appears on your console's screen. You can begin configuration. .

## Related Documentation

- Setting Up Management Access on the CTP2000 Platform
- CTP2000 Console Port Setup
- Using HyperTerminal with the CTP2000 Platform
- CTP2000 Platform SSH Setup

#### Published: 2010-09-30

﻿
Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out