Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

## Related Documentation

- Circuit Startup Process Overview

# Configuring Circuit Startup Parameters for CTP Bundles (CTP Menu)

This topic describes how to configure advanced options are related to circuit startup. Set these parameters to the same values on the local and remote CTP devices.

Before you begin:

- Disable the bundle before you modify the bundle options.

To configure circuit startup parameters using the CTP Menu:

1. From the Main Menu, select 1) Bundle Operations.
2. Select 1) CTP.
3. Select a bundle from the list.

   If you select an active bundle, you are prompted to disable the bundle before configuring it.

4. Select 2) Config.
5. Select 10) Advanced Options.
6. Configure options 4, 5, 6, 7, and 8 as described in Table 1.

Field | Function | Your Action
--- | --- | ---
Consecutive pkts loss to starve | Specifies how many consecutive circuit packets the IP network must drop before the CTP device restarts the circuit. We recommend that you set the parameter to a larger value when the IP network uses packet-encrypting devices. These devices cause momentary interruption in packet flows when encryption keys are updated. | Enter a number from 1 through 64.
In sequence pkts after starve | Specifies the number of in-sequence packets the CTP device must receive after a starvation before the circuit transitions from in-sync to running. | Enter a number from 1 through 64.
OAM Chan Rate (pkt/sec) | Specifies the number of OAM packets per second that the circuit sends to the remote CTP device. | Enter a number from 1 through 255.
OAM pkts for Sync | Specifies the number of OAM packets that the circuit must receive before the state moves from no synchronization to in synchronization. | Enter a number from 1 through 255.
OAM pkts for Sync Loss | Specifies the number of received OAM packets that the CTP device misses before the state of the circuit moves from in synchronization to no synchronization. | Enter a number from 1 through 255.

## Related Documentation

- Circuit Startup Process Overview

#### Published: 2011-01-09

﻿
Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out