Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

## Related Documentation

- Adaptive Clocking Overview for CTP Bundles

# Configuring Adaptive Clocking for CTP Bundles (CTP Menu)

The adaptive clocking configuration allows you to modify attributes that affect the adaptive clocking algorithm. The default settings are acceptable for most applications. We recommend that you change these settings only with the assistance of JTAC.

Before you begin:

- Disable the bundle before you modify the bundle options.

To configure adaptive clocking for CTP bundles using the CTP Menu:

1. From the Main Menu, select 1) Bundle Operations.
2. Select 1) CTP.
3. Select a bundle from the list.

   If you select an active bundle, you are prompted to disable the bundle before configuring it.

4. Select 3) Port Config.
5. Select 3) Clock Config.
6. Select 1) Port Clock Config.
7. Select Set Adaptive Parameters.
8. Configure the options as described in Table 1.

Field | Function | Your Action
--- | --- | ---
Set to Defaults | Sets the adaptive clocking configuration to the default settings. | Select Set to Defaults.
AGGR Seconds/Calc | Specifies the time period during initial start of adaptive clocking during which packet samples that are experiencing the least delay through the network are collected. These samples are used for aggressive state calculations. | Enter a number from 3 through 200 seconds.
MNTN Seconds/Calc | Specifies the time period during normal adaptive clocking during which packet samples that are experiencing the least delay through the network are collected. These samples are used for maintenance state calculations. | Enter a number from 3 through 300 seconds.
Slope for MNTN in ppm | Specifies the number of packets per minute, which when reached, causes the adaptive clocking algorithm to change from aggressive state to maintenance state. Lower values result in longer switchover times with a clock value closer to the remote clock. | Enter a number from 1 through 100 packets per minute.
Maintenance Decay in calcs | Specifies how quickly the clocking corrects to the buffer set point while in maintenance state. | Enter a number from 2 though 120 seconds.
Max Clock Adjust in ppb | Specifies a cap for frequency acceleration, which constrains the frequency adjustments to the adaptive clock. | Enter a number from 1 through 1000 parts per billion.
Max Clock Offset in ppm | Specifies a cap for frequency velocity, which constrains the frequency velocity of the adaptive clock. | Enter a number from 1 through 400 packets per minute.
Max Buffer Error in usec | Specifies the buffer error rate required to change the adaptive clocking algorithm state from maintenance to aggressive. | Enter a number from 100 through 1,000,000 ųsec.

## Related Documentation

- Adaptive Clocking Overview for CTP Bundles

#### Published: 2011-01-09

﻿
Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out