Country

- China
- France
- Germany
- Japan
- Korea
- Spain
- Taiwan
- United Kingdom
- United States

Contact Us
|
Country
United States

# Technical Documentation

- Download Software
- Research a Problem
- Case Management
- Contract & Product Management
- Technical Documentation
  - Advanced Search
  - Documentation Archive
  - Documentation Bug Report
  - Enterprise MIBs
  - File Format Help
  - Glossary
  - Portable Libraries
- End-of-Life Products
- Contact Support
- Guidelines and Policies
- Security Resources

- Downloads
- CTP2000 Series T1/E1 Interface Module

- Related Topics
- CTP2000 Series Serial Interface Modules
- CTP2000 Compression Interface Module
- CTP2000 4W&EM Interface Module
- CTP2000 2W-FXS and 2W-FXO Interface Modules
- CTP2000 8P-IRIG Interface Module

# CTP2000 Series T1/E1 Interface Module

The CTP2000 Series T1/E1interface module has RJ-48 ports numbered 0–7 left to right. It provides a configurable eight-port E1 (2.048 MHz) or T1 (1.544 MHz) interface with AMI or B8ZS encoding. (See Figure 1.)

Figure 1: CTP2000 IM-8P-T1/E1 Interface Module

#### Published: 2010-05-11