Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

## Related Documentation

- Gain Control for Analog Voice Modules Overview
- 4WE&M Interface Module with VComp Bundles Overview

# Configuring 4WE&M Port Parameters for VComp Bundles (CTPView)

This topic describes how to configure port parameters for 4WE&M interfaces.

Before you begin:

- Log in to the CTPView software at least at the Net_Admin level.
- Connect the CTPView server to the CTP device for which you want to configure bundles.
- Disable the bundle before you modify the bundle options.

To configure port parameters for 4WE&M interfaces using CTPView:

1. In the side pane, select Bundle > Configuration.
2. Run your mouse over the Display and Select an Existing Bundle bar.
3. In the table of bundles, select the bundle that you want to modify.
4. Under Port Options, configure the parameters described in Table 1.
5. Click Click to Submit Bundle AND Port Changes.

Table 1: VComp Bundle 4WE&M Port Parameter Settings in CTPView

Field | Function | Your Action
--- | --- | ---
Voice Port Tx Gain [ -23.8 to 1.6 dB ] | Specifies the gain in the direction from the analog interface toward the IP network. | Select a dB value from the list.
Voice Port Rx Gain [ -7.6 to 17.7 dB ] | Specifies the gain in the direction from the IP network to the analog interface. | Select a dB value from the list.

## Related Documentation

- Gain Control for Analog Voice Modules Overview
- 4WE&M Interface Module with VComp Bundles Overview

#### Published: 2010-10-27

﻿
Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out