Country

- China
- France
- Germany
- Japan
- Korea
- Spain
- Taiwan
- United Kingdom
- United States

Contact Us
|
Country
United States

# Technical Documentation

- Download Software
- Research a Problem
- Case Management
- Contract & Product Management
- Technical Documentation
  - Advanced Search
  - Documentation Archive
  - Documentation Bug Report
  - Enterprise MIBs
  - File Format Help
  - Glossary
  - Portable Libraries
- End-of-Life Products
- Contact Support
- Guidelines and Policies
- Security Resources

- Downloads
- CTP1012 Platform

- Related Topics
- CTP1002 Platform
- CTP1004 Platform

# CTP1012 Platform

The CTP1012 platform is a 1-U high, full-rack wide chassis designed for tabletop or shelf installation. It can also be installed in a rack with the supplied rack-mounting kit. The CTP1012 device does not have any removable interface modules, but does use a removable Type II CompactFlash card and is available in an AC-powered version. It has multiple cooling fans, and airflow is front to back. See Figure 1 and Figure 2.

Figure 1: CTP1012 Platform (AC Version, Front View)

The front panel comprises the following components (see Figure 1):

- Power LED—Green when power is connected and the power switch is set to the ON position.
- HDD LED—Red when the flash card is in use.
- Front power switch—Set to ON position when 1 is briefly pressed. Set to OFF when 1 is pressed for four or more seconds.
- Removable flash card—The device must be powered off when you insert or remove the flash card.
- USB ports.

The rear panel comprises the following components (See Figure 2):

- Power supply—Uses a standard IEC power cord.
- Ethernet connection—Provides the 100-Mbps Ethernet connection to the IP network by means of a local Ethernet switch or router.
- Console connection—Provides an asynchronous TTY connection for locally configuring the CTP device. See CTP1000 Console Cable Pinouts to find pinout information for this connector.
- Interface connector—Features a 100-pin connector providing four serial interfaces when used with the CTP quad cable. SeeCTP1000 Interface Module 100-to-25-Pin Cable Pinouts to find pinout information for this connector.
- USB ports.

Figure 2: CTP1012 Platform (AC Version, Rear View)

#### Published: 2010-05-11