Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

## Related Documentation

- Bundle Failover Between CTP Devices at Alternate Sites Overview
- Configuring Bundle Failover Between CTP Devices at Alternate Sites (CTPView)

# Checking Primary and Secondary AutoSwitch Connections for Bundles (CTPView)

You can test the connection between a CTP device running AutoSwitch and its primary and secondary circuits.

Before you begin:

- Log in to the CTPView software at least at the Net_Admin level.
- Connect the CTPView server to the CTP device on which you want to use this feature.

To test connections to primary and secondary circuits using CTPView:

1. In the side pane, select System > Configuration.
2. Click AutoSwitch.
3. Under Connection Check, you have the option of verifying all connections or verifying specific connections.
   - To verify all connections, under Connection Check, click ALL.
   - To verify connections for a specific primary or secondary circuit, click Test under the Primary Host and Secondary Host columns.

   During the test, the buttons turn blue and display Testing. The results of the test are displayed inside the buttons, and the background color around the buttons either turns green for success or red for failure.

## Related Documentation

- Bundle Failover Between CTP Devices at Alternate Sites Overview
- Configuring Bundle Failover Between CTP Devices at Alternate Sites (CTPView)

#### Published: 2010-10-26

﻿
Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out