Country

- China
- France
- Germany
- Japan
- Korea
- Spain
- Taiwan
- United Kingdom
- United States

Contact Us
|
Country
United States

# Technical Documentation

- Download Software
- Research a Problem
- Case Management
- Contract & Product Management
- Technical Documentation
  - Advanced Search
  - Documentation Archive
  - Documentation Bug Report
  - Enterprise MIBs
  - File Format Help
  - Glossary
  - Portable Libraries
- End-of-Life Products
- Contact Support
- Guidelines and Policies
- Security Resources

- Downloads
- CTP1000 Mechanical Requirements

- Related Topics
- CTP1000 Rack Requirements
- CTP1000 Space Requirements
- CTP1000 Rack Installation

# CTP1000 Mechanical Requirements

Follow these mechanical requirements for your rack:

- Select from the following rack options:
  - Two-post rack—A freestanding enclosed cabinet with two mounting posts in the front
  - Telco-type rack—Two adjacent mounting posts that you must secure to the floor or an overhead structure
  - Four-post rack—A freestanding open rack, either open or closed
- The rack must have at least two mounting posts.
- The distance between the mounting holes in the two posts must be 18.31 in. ±.063 in., as specified in the EIA-310-D document.
- An optional mounting kit is available for midchassis mounting. Contact your Juniper Networks sales representative for more information.

#### Published: 2010-05-11