Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

## Related Documentation

- Connecting Directly to the CTP150 Platform
- Using HyperTerminal to Access the CTP150 Device
- Using SSH to Access the CTP Platform

# Setting Up Management Access to the CTP150 Platform

Before you power on the device for the first time, you need to physically connect a console (PC, Macintosh, or UNIX workstation) to the device’s CONSOLE port. Through this connection, you communicate with the CTP150 device during the power-on process to set an IP address and initially configure the device.

After you configure an IP address on the CTP150 device, you can access the device remotely through the Ethernet port by running SSH from a remote console.

## Related Documentation

- Connecting Directly to the CTP150 Platform
- Using HyperTerminal to Access the CTP150 Device
- Using SSH to Access the CTP Platform

#### Published: 2011-01-31

﻿
Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out