Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

## Related Documentation

- SAToP Bundle Overview

# Configuring Virtual IP Parameters for SAToP Bundles (CTP Menu)

The virtual IP parameters allow you to use a separate IP address for each bundle and to use an address that is different from the IP address for the CTP device. If you configure the IP address on the:

- Same subnet as the CTP IP address, you do not need a static route on the router.
- Different subnet as the CTP IP address, you need a static route on the router.

Before you begin:

- Create a list of the virtual IP addresses that will be associated with the CTP device. To do so, from the main menu select Node Operations > Configure network settings > Virtual IP addresses, and follow the onscreen instructions.

  When you submit your new configuration, the CTP device reboots.

- Disable the bundle before you modify the bundle options.

To configure virtual IP parameters for SAToP bundles using the CTP Menu:

1. From the Main Menu, select 1) Bundle Operations.
2. Select 2) SAToP.
3. Select a bundle from the list.

   If you select an active bundle, you are prompted to disable the bundle before configuring it.

4. Select 2) Config.
5. Select 10) Advanced Options.
6. Configure the options as described in Table 1.

Field | Function | Your Action
--- | --- | ---
Use virtual ip for port | Specifies whether or not the bundle uses an address that is different from the IP address of the CTP device. The virtual IP address is used in the IP packet’s Origination Address field, and is used for the circuit’s data and OAM flow. | Select one: n (no)—Circuits created by this bundle use the IP address of the CTP device. y (yes)—Circuits created by this bundle use an address that is different from the CTP device.
Virtual ip for port | Specifies the virtual IP address for circuits created by this bundle. | Select an IP address from the list displayed. At the remote end of the bundle, specify this IP address as the Remote Address of the bundle.

## Related Documentation

- SAToP Bundle Overview

#### Published: 2010-10-21

﻿
Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out