Country

- China
- France
- Germany
- Japan
- Korea
- Spain
- Taiwan
- United Kingdom
- United States

Contact Us
|
Country
United States

# Technical Documentation

- Download Software
- Research a Problem
- Case Management
- Contract & Product Management
- Technical Documentation
  - Advanced Search
  - Documentation Archive
  - Documentation Bug Report
  - Enterprise MIBs
  - File Format Help
  - Glossary
  - Portable Libraries
- End-of-Life Products
- Contact Support
- Guidelines and Policies
- Security Resources

- Downloads
- CTP1000 Console Port Setup

- Related Topics
- Setting Up Management Access on the CTP1000 Platform

# CTP1000 Console Port Setup

You can connect a console terminal (PC, Macintosh, or UNIX workstation) through the RS-232 terminal port. When you connect a console directly to the device, you can configure the device without an IP address.

To communicate with the device, you must have a terminal emulation program running on your PC or Macintosh. You can use any terminal emulation program, such as HyperTerminal. A UNIX workstation can use the emulator TIP.

#### Published: 2010-05-11