Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

## Related Documentation

- CTP Fast Ethernet and Power Cables

# CTP150 Console Cable Pinouts

The console connector to the CTP150 platform is a standard RJ-45 to DB-9 adapter cable. Figure 1 displays the console cable pin configurations for CTP150 device. On the left is the RJ-45 connector, and on the right is the DB-9 connector with the pin numbering indicated.

The console connections are configured to the following parameters:

- Speed: 9600 bps
- Data bits: 8
- Stop bits: 1
- Flow control: Xon/Xoff
- Parity: none

Figure 1: CTP150 Console Cable Pin Configurations

Table 1 lists console cable pinouts for the CTP150 device based on the pin configurations.

Table 1: CTP150 Series Console Cable Pinouts

CTP RJ-45 Pin | Console DB-9 Pin
--- | ---
1 RTS | 8 CTS
2 DTR | 6 DSR
3 TXD | 2 RXD
4 GND | 5 GND
5 GND | 5 GND
6 RXD | 3 TXD
7 DSR | 4 DTR
8 CTS | 7 RTS

## Related Documentation

- CTP Fast Ethernet and Power Cables

#### Published: 2011-01-31

﻿
Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out