Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

## Related Documentation

- Installing a CTP Interface Module, Processor Module, or Clock Module

# Installing a PMC on CTP2000 Platforms

The PCI mezzanine card (PMC) is mounted on the processor module and can be installed or replaced in the field. Figure 1 displays the location of the PMC.

Figure 1: CTP2000 Platforms PMC Location

To install a PMC:

1. Confirm that the device is powered off.
2. Remove the RTM by unscrewing the retaining screws and pushing the extractors outward while depressing the latching buttons.
3. If a PMC was not previously installed, a shield may have been inserted in the PMC slot of the processor’s front panel. Remove this shield by gently pushing it out from behind the panel.
4. The PMC has four screws. Two of the screws are secured to standoffs, and two are attached to the front assembly of the PMC. Remove the two screws secured to the standoff, leaving the standoff attached to the PMC. Remove the two screws on the front assembly located on the side with the standoffs. The front assembly should remain attached to the PMC hardware. Keep the screws for reattachment.
5. Align the PMC with the printed circuit board connectors toward the processor board and with the fiber connectors inserted through the processor’s front panel. Align the alignment post on the processor module with the PMC’s alignment hole.
6. Gently press the PMC into the processor module.
7. From the back of the processor module, use the four Phillips head screws to secure the two PMC standoff posts and PMC front assembly to the processor module.
8. Reinstall the processor RTM in the reverse procedure of removing it. Be sure that the screws and latching are secure

## Related Documentation

- Installing a CTP Interface Module, Processor Module, or Clock Module

#### Published: 2010-09-30

﻿
Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out