Log in
|
How to Buy
|
Contact Us
|
United States (Change)

## Choose Country

### North America

- United States

### Europe

- Deutschland - Germany
- España - Spain
- France
- Italia - Italy
- Россия - Russia
- United Kingdom

### Asia Pacific

- Asean Region (Vietnam, Indonesia, Singapore, Malaysia)
- Australia
- 中国 - China
- India
- 日本 - Japan
- 대한민국 - Korea
- 台灣 - Taiwan

Remember my choice

# Technical Documentation

Download Software
Research a Problem
Case Management
Contract & Product Management
Technical Documentation
Documentation Archive
Report Documentation Bug
Enterprise MIBs
File Format Help
Glossary
Portable Libraries
End-of-Life Products
Contact Support
Guidelines and Policies
Security Resources
Feedback

## Documentation Search

Advanced Search | Search Tips

# Configuring Advanced Port Options for CTP Bundles (CTP Menu)

Before you begin:

- Disable the bundle before you modify the bundle options.

To configure advanced port options for CTP bundles using the CTP Menu:

1. From the Main Menu, select 1) Bundle Operations.
2. Select 1) CTP.
3. Select a bundle from the list.

   If you select an active bundle, you are prompted to disable the bundle before configuring it.

4. Select 3) Port Config.
5. Select 4) Advanced Options.
6. Configure the options as described in Table 1.

Field | Function | Your Action
--- | --- | ---
Single ended data/clock outputs | Do not change this value without consulting JTAC. Specifies whether or not the CTP device drives received data (RD) onto data set ready (DSR) and real-time (RT) data onto test mode (TM). | Select y or n.
Reclock RD to align RD/RT | Do not change this value without consulting JTAC. Specifies whether or not to reclock RD with the RT clock to align the data and the clock. | Select y or n.
Only high TT checking | Specifies that the CTP device disqualifies transmit timing (TT) only when it is higher than the port speed. When enabled, this setting keeps the port from going to the TtFail state when the incoming user clock fluctuates between 0 and the configured port rate. If the TT rate goes above the configured port rate, the CTP device sends the port to the TtFail state to protect the system from an overspeed TT, which would cause problems for the port, CTP device, or network. | Select y or n.
TT Clock Gated by RTS | When request to send (RTS) is inactive, specifies whether or not the CTP device feeds TT with the internally created clock. | Select y or n.
RTS Clock Gate Invert | When clock gating is enabled, specifies whether or not to use the inverted RTS signal. | Select y or n.
Input/Output Data Invert | Specifies whether or not to invert data bound for the interface with data bound for the IP network. | Select y or n.

#### Published: 2011-01-09

﻿
Site Map / RSS Feeds / Careers / Accessibility / Feedback / Privacy & Policy / Legal Notices
Copyright© 1999-2011 Juniper Networks, Inc. All rights reserved.
Help
|
My Account
|
Log Out